Stopped initial reset

blockreset basic

Started watch 1 Count

laptime 2

display

storerecall_control 3

actual stored

display 4

display

[run]

[!run]

[store]

2

[!store] 1

[store]

[!store] / minutes = 0; min = 0; seconds = 0; sec = 0

[!store] / min = minsave; minutes = minsave; sec = secsave; seconds = secsave

tick [sec == 599] / min = min +1; sec = 0; ticklap 1 tick [sec < 599] / sec := sec + 1; ticklap 2

ticklap [lap ==0] / dmin = min; dsec = sec; tickdisplay

[store] / minsave = minutes; secsave = seconds;

[!store] / min = minsave; minutes = minsave; sec = secsave; seconds = secsave

tickdisplay [lap ==0] / minutes = dmin/10; seconds = dsec/ 10